RTI CX10 Firmware Version 20.8.25

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 20.8.25 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer or Integration Designer
to determine the current firmware version. The reported version number
will consist of a number followed by a bootloader version number
[for example: 20.8.25 (Bootloader: 1.3)]. If the first part of the reported
version number is 20.8.25 or higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher, or Integration Designer 6.0 or
higher must already be installed on the PC that you wish to use to
upgrade the CX10 firmware.  If your PC runs a 64-bit version of Windows,
Integration Designer 7.0 must be installed to perform the upgrade.
Upgrading to the latest version of Integration Designer is strongly
recommended.  You should verify that you can communicate with the CX10
using Integration Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Connect power to the CX10 and make sure it operates normally.
2. Make sure Integration Designer 6.0 or higher is installed on the
   PC that you are using to update the CX10 firmware, and that Integration
   Designer can communicate successfully with the CX10.  You can use the
   "Get Firmware Version" command on the Communications menu in Integration
   Designer to verify that the USB communications are working properly.
3. Run the CX10Update_20.8.25.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

LIST OF CHANGES IN THIS RELEASE (RELEASE 20.8.25)
- Improved reliability of the system file downloads and firmware upgrades
- Improved network reliability in certain environments
- Fixed intermittent dynamic image loading over SSL
- Improved overall system performance

LIST OF CHANGES IN RELEASE 2.0.5
- Improved reliability of Firmware Updates and System Downloads.
- Fixed firmware updates from computers with multiple network adapters.
- Prevented CX-10 from getting into a continuous boot cycle.
- Fixed Composite Video for PAL

LIST OF CHANGES IN RELEASE 1.2.11
- Added RTSP/H.264 streaming support
- Fixed misc. VoIP issues
- Improved PNG decoding reliability

LIST OF CHANGES IN RELEASE 1.1.5
- Added the ability to update firmware over the network
- Improved image decoding reliability (GIF,PNG,JPG)