RTI KA 8 & 11 Firmware Version 2.0.27


INTEGRATION DESIGNER SUPPORT
Use the latest version of Integration Designer to perform this update.


FIRMWARE UPGRADE PROCEDURE
1. Choose the "Update Firmware" command on the Communications menu in
   Integration Designer.
2. Select the .RFW file included with this README file.
3. Make sure you have your program saved (see the WARNING above), then
   click OK.
4. Make sure the KA device is connected to the same LAN as the PC running 
   Integration Designer and select the KA device in the Network section of
   the Select Update Method screen.  The firmware update process will start.
5. If there's also an additional firmware update available online, you'll be
   prompted to accept the update or not.  Updating is required to enable
   new features.  Note: the update will take several minutes to download
   and complete.
6. Wait for the KA device to reset.


LIST OF CHANGES IN RELEASE (2.0.27)
1. Added VoIP support


LIST OF CHANGES IN RELEASE (1.1.6)
1. Added static IP address support
2. Added backlight dimming support
3. Added proximity sensor support
4. Added ambient light sensor support
5. Removed WiFi support
