RTI KX7 Firmware Version 20.8.25

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 20.8.25 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer or Integration Designer
to determine the current firmware version. The reported version number
will consist of a number followed by a bootloader version number
[for example: 20.8.25 (Bootloader: 2.0)]. If the first part of the reported
version number is 20.8.25 or higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher, or Integration Designer 6.0 or
higher must already be installed on the PC that you wish to use to
upgrade the KX7 firmware.  If your PC runs a 64-bit version of Windows,
Integration Designer 7.0 must be installed to perform the upgrade.
Upgrading to the latest version of Integration Designer is strongly
recommended.  You should verify that you can communicate with the KX7
using Integration Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Connect power to the KX7 and make sure it operates normally.
2. Make sure Integration Designer 6.0 or higher is installed on the
   PC that you are using to update the KX7 firmware, and that Integration
   Designer can communicate successfully with the KX7.  You can use the
   "Get Firmware Version" command on the Communications menu in Integration
   Designer to verify that the USB communications are working properly.
3. Run the KX7Update_20.8.25.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

LIST OF CHANGES IN THIS RELEASE (RELEASE 20.8.25)
- Improved reliability of the system file downloads and firmware upgrades
- Improved network reliability in certain environments
- Fixed intermittent dynamic image loading over SSL
- Improved overall system performance

LIST OF CHANGES IN RELEASE 2.0.5
- Improved reliability of Firmware Updates and System Downloads.
- Fixed firmware updates from computers with multiple network adapters.
- Fixed Composite Video for PAL

LIST OF CHANGES IN RELEASE 1.8.11
- Added RTSP/H.264 streaming support
- Fixed misc. VoIP issues
- Improved PNG decoding reliability

LIST OF CHANGES IN RELEASE 1.7.5
- Added the ability to update firmware over the network
- Added support for VoIP SIP Server Registration
- Added support for MJPEG Digest Authentication
- Improved image decoding reliability (GIF,PNG,JPG)

LIST OF CHANGES IN RELEASE 1.6.5
- VoIP Video support
- Improved VoIP DTMF reliability

LIST OF CHANGES IN RELEASE 1.4.21
- Added VoIP Intercom support
- MJPEG stability and compatibility improvements
- Fix for variable Reversed State not considering initial Reversed state
- Fix for HTTPS URLs not loading

LIST OF CHANGES IN RELEASE 1.2.53
- Fix for two-way scrolling list refresh issue
- Fix for instability issues when displaying very small analog video windows
- Fix for instability issues when using Analog Video Viewer Select Input commands
- Fix for Prevent Backlight Power Down issues when using Analog Video Viewer Select Input commands
- Fix for 480i video quality issues
- Fix for issue with sliders not allowing selection of -1
- Allow horizontal frame gestures when initial press is on a vertical slider
- Hide MJPEG windows when in full screen video mode

LIST OF CHANGES IN RELEASE 1.1.11
- Support for one-way RS-232 control
- Support for CPB-1
- Improved dithering and translucent button rendering
- Support for Allow Full Screen Mode of Analog Video Viewer
- Fix for Analog Video Viewer playback quality issues
- Fix for Analog Video Viewer stability issue when clicking on overlapping buttons
- Increased maximum sysvars per page
- Support for Ignore First Press from Power Down Mode
- Support for horizontal frame gesturing on scrolling lists
- Fixes for scrolling lists marked as Show On All Frames
- Fix for WiFi networks set to not broadcast SSID
- Fixes for Control Panel WiFi Network information display
