RTI Pro24.z Firmware Version 1.5.1

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 1.5.1 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in Integration Designer to determine the current
firmware version. The reported version number will consist of a number
followed by a bootloader version number [for example: 3.0 (Bootloader:
1.3)]. If the first part of the reported version number is 1.5.1 or
higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
Integration Designer APEX 10.2 or higher must already be installed on the
PC that you wish to use to upgrade the Pro24.z firmware. Upgrading to the
latest version of Integration Designer APEX is strongly recommended.  You
should verify that you can communicate with the Pro24.z using Integration
Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Make sure the battery on the Pro24.z is fully charged.  The Pro24.z may be left
   inoperable if the battery fails during the firmware update.
2. Make sure Integration Designer APEX 10.2 or higher is installed on the
   PC that you are using to update the Pro24.z firmware, and that Integration
   Designer can communicate successfully with the Pro24.z.  You can use the
   "Get Firmware Version" command on the Communications menu in Integration
   Designer to verify that the USB communications are working properly.
3. Run the PRO24ZUpdate_version#.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.
