RTI RK3 Firmware Version 2.4

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 2.4 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer or Integration Designer
to determine the current firmware version. The reported version number
will consist of a number followed by a bootloader version number
[for example: 2.4 (Bootloader: 1.3)]. If the first part of the reported
version number is 2.4 or higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher, or Integration Designer 6.0 or
higher must already be installed on the PC that you wish to use to
upgrade the RK3 firmware.  If your PC runs a 64-bit version of Windows,
Integration Designer 7.0 must be installed to perform the upgrade.
Upgrading to the latest version of Integration Designer is strongly
recommended.  You should verify that you can communicate with the RK3
using Integration Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Connect power to the RK3 and make sure it operates normally.
2. Make sure TheaterTouch Designer 3.0 or higher or Integration
   Designer 6.0 or higher is installed on the PC that you are using to
   update the RK3 firmware, and that Integration Designer can communicate
   successfully with the RK3.  You can use the "Get Firmware Version"
   command on the Communications menu in Integration Designer to verify
   that the USB communications are working properly.
3. Run the rk3update.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

ENABLING FLASH PLAYER SUPPORT
This firmware update includes support for displaying Adobe Flash
content in the web browser. If the RK3 was not shipped from the factory
with Flash support enabled, you must run the included FlashEnable.exe
utility and follow the directions on-screen to enable the Flash
player after you have performed the firmware update. This procedure
only needs to be done once per RK3, it will not have to be done after
future firmware updates.

LIST OF CHANGES IN THIS RELEASE (RELEASE 2.4)
1. Fix for weather radar images not updating.
2. Two-way itemlist enhancements.

LIST OF CHANGES IN RELEASE 2.2
1. Updated Daylight Saving Time start and end dates for Australia.
2. Added support for VIVOTEK and Y-cam MJPEG cameras. (*)
3. Fix bug that could cause lockup when using a standalone macro with
   two or more system macro triggers.
4. Fix a number of potential lockups when using the web browser object.

(*) NOTE: Integration Designer 7.2.2 or higher is required to use this feature.

LIST OF CHANGES IN RELEASE 2.1
1. Added support for triggering sounds remotely. (*)
2. Added support for returning the backlight to its active level when
   a remotely-triggered page link is received. (*)
3. Added support for scrolling text fields. (*)
4. Added support for RS-485 communications to compatible control
   processors. (*)
5. Added support for using local flag states as system variables. (*)
6. Added support for controlling Power LED with system variables. (*)
7. GIF / Animated GIF support added for Dynamic Images.
8. Fixed bug that caused "Wait for macro to finish" property to be
   ignored when calling system macros from within a standalone macro.
   The standalone macro will now wait for each system macro to finish
   before continuing if that macro is triggered with a two-way transport
   on a two-way processor. The old behavior can be preserved by un-checking
   the "Wait for macro to finish" on the button properties.
9. Fixed bug that would cause sustain to stop when using volume popup.

(*) NOTE: Integration Designer 7.1 or higher is required to use this feature.


LIST OF CHANGES IN RELEASE 2.0
1. Added two-way communications support.  Integration Designer 7.0 or
   higher is required to use this feature.
2. Fixed bug that caused problems reading the state of the local power
   and aux status ports from inside a macro.
3. Fixed bug that caused all URLs in HTTP Request and MJPEG viewer
   objects that specified an explicit port to have an 80 prefix added.
   NOTE: Any programs containing MJPEG viewer windows that specify a port
   number explicitly will have to be changed to work with this version.
   For example, if the MJPEG viewer object is set to port 81 in the previous
   version, it will have to be changed to 8081 to work with this version.
4. Restore backlight settings properly after firmware update.

LIST OF CHANGES IN RELEASE 1.3
1. Added support for CPB-1.
2. Added support for disabling on-screen keyboard when using Web Browser
   Objects.  Integration Designer 6.1 or higher is required to use
   this option.

LIST OF CHANGES IN RELEASE 1.2
1. Added Adobe Flash Player support to Web Browser.

LIST OF CHANGES IN RELEASE 1.1
1. Updated Daylight Saving Time clock adjustment dates for 2007 and beyond.
2. Added scrolling list support. (*)
3. Fixed bug that could cause a crash when using MJPEG video objects
   with 240x180 video size.
4. Fixed issue that prevented clock from being synchronized with NTP servers
   in some cases.
5. Added options to control the display of the address bar and scroll bar
   in the Web Browser object. (*)
6. Added options to assign commands to the hardkeys that cause the web browser
   object to scroll. (*)
7. Fixed issue that could cause the Web Browser object to crash when
   rendering certain web pages.
8. Improved Web Browser compatibility with web sites that use the
   XMLHttpRequest object.

(*) Requires TheaterTouch Designer 5.0 or higher