RTI RK3-V Firmware Version 1.4

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 1.4 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer or Integration Designer
to determine the current firmware version. The reported version number
will consist of a number followed by a bootloader version number
[for example: 1.4 (Bootloader: 1.3)]. If the first part of the reported
version number is 1.4 or higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher, or Integration Designer 6.0 or
higher must already be installed on the PC that you wish to use to
upgrade the RK3-V firmware.  If your PC runs a 64-bit version of Windows,
Integration Designer 7.0 must be installed to perform the upgrade.
Upgrading to the latest version of Integration Designer is strongly
recommended.  You should verify that you can communicate with the RK3-V
using Integration Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Connect power to the RK3-V and make sure it operates normally.
2. Make sure TheaterTouch Designer 3.0 or higher or Integration
   Designer 6.0 or higher is installed on the PC that you are using to
   update the RK3 firmware, and that Integration Designer can communicate
   successfully with the RK3-V.  You can use the "Get Firmware Version"
   command on the Communications menu in Integration Designer to verify
   that the USB communications are working properly.
3. Run the rk3vupdate.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

LIST OF CHANGES IN THIS RELEASE (RELEASE 1.4)
1. Fix for weather radar images not updating.
2. Fix for IR receiver not working.
3. Two-way itemlist enhancements.

LIST OF CHANGES IN RELEASE 1.2
1. Fixed bug that caused static IP address settings to be ignored.

LIST OF CHANGES IN RELEASE 1.1
1. Updated Daylight Saving Time start and end dates for Australia.
2. Added support for VIVOTEK and Y-cam MJPEG cameras. (*)
3. Fix bug that could cause lockup when using a standalone macro with
   two or more system macro triggers.
4. Fix a number of potential lockups when using the web browser object.

(*) NOTE: Integration Designer 7.2.2 or higher is required to use this feature.

LIST OF CHANGES IN RELEASE 1.0
* Initial production release
