RTI T2-C Firmware Version 2.4

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 2.4 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer or Integration Designer
to determine the current firmware version. The reported version number
will consist of a number followed by a bootloader version number
[for example: 2.4 (Bootloader: 1.3)]. If the first part of the reported
version number is 2.4 or higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher, or Integration Designer 6.0 or
higher must already be installed on the PC that you wish to use to
upgrade the T2-C firmware.  If your PC runs a 64-bit version of Windows,
Integration Designer 7.0 must be installed to perform the upgrade.
Upgrading to the latest version of Integration Designer is strongly
recommended.  You should verify that you can communicate with the T2-C
using Integration Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Make sure the battery on the T2-C is fully charged.  The T2-C may be left
   inoperable if the battery fails during the firmware update.
2. Make sure TheaterTouch Designer 3.0 or higher is installed on the PC
   that you are using to update the T2-C firmware, and that TheaterTouch
   Designer can communicate successfully with the T2-C.  You can use the
   "Get Firmware Version" command on the Communications menu in
   TheaterTouch Designer to verify that the USB communications are
   working properly.
3. Run the t2cupdate.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

LIST OF CHANGES IN THIS RELEASE (RELEASE 2.4)
1. Fix for double-hit issue when using 433.
2. Two-way itemlist enhancements.

LIST OF CHANGES IN RELEASE 2.2
1. Fix bug that could cause lockup when using a standalone macro with
   two or more system macro triggers.
2. Extend ZigBee disconnect time to 5 days (up from 30 minutes).
3. Add manual ZigBee reconnect support. (*)

(*) NOTE: Integration Designer 7.2.2 or higher is required to use this feature.

LIST OF CHANGES IN RELEASE 2.1
1. Added support for triggering sounds remotely. (*)
2. Added support for scrolling text fields. (*)
3. Added support for using local flag states as system variables. (*)
4. GIF / Animated GIF support added for Dynamic Images.
5. Fixed bug that caused "Wait for macro to finish" property to be
   ignored when calling system macros from within a standalone macro.
   The standalone macro will now wait for each system macro to finish
   before continuing if that macro is triggered with a two-way transport
   on a two-way processor. The old behavior can be preserved by un-checking
   the "Wait for macro to finish" on the button properties.
6. Fixed bug that would cause sustain to stop when using volume popup.
7. Fixed issue that would occasionally cause long delays with Zigbee
   reconnection after downloading a new program to the device.

(*) NOTE: Integration Designer 7.1 or higher is required to use this feature.


LIST OF CHANGES IN RELEASE 2.0
1. Added two-way communications support.  Integration Designer 7.0 or
   higher is required to use this feature.
2. Add support for Zigbee-enabled hardware.
3. Add support for the "Don't save source page in history" page link option.
4. Added support for text in Simplified and Traditional Chinese
   character sets.
5. Fixed bug that caused certain unusually-formatted IR codes to lock up
   the T2-C when transmitted.
