RTI T3 Firmware Version 1.6

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 1.6 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer to determine the
current firmware version. The reported version number will consist of
two numbers separated by a slash [for example: 1.6 / 1.3] if you are
using TheaterTouch Designer 5.0 or earlier, or a number followed by
a bootloader version number [for example: 1.6 (Bootloader: 1.3)] if
you are running TheaterTouch Designer 5.01 or higher. If the first
part of the reported version number is 1.6 or higher, you do
not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher must already be installed on the
PC that you wish to use to upgrade the T3 firmware.  You should verify
that you can communicate with the T3 using TheaterTouch Designer before
attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Verify that the T3 battery is fully charged. If the low battery
   icon appears, charge the battery before proceeding with this update.
2. Make sure TheaterTouch Designer 3.0 or higher is installed on the PC
   that you are using to update the T3 firmware, and that TheaterTouch
   Designer can communicate successfully with the T3.  You can use the
   "Get Firmware Version" command on the Communications menu in
   TheaterTouch Designer to verify that the USB communications are
   working properly.
3. Run the t3update.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

LIST OF CHANGES IN THIS RELEASE (RELEASE 1.6)
1. Fixed issue that could cause the tilt switch on a small number of T3
   units to stop responding until the unit was power-cycled.

LIST OF CHANGES IN RELEASE 1.5
1. Fixed issue that could cause T3 units shipped from the factory with
   firmware release 1.3 to lock up in some istuations when running macros
   in IR Standalone mode.  This fix is an improvement on the one included
   in firmware release 1.4 that fixes a few situations that were not
   covered by the 1.4 update.

LIST OF CHANGES IN RELEASE 1.4
1. Fixed issue that could cause T3 units running firmware release 1.3 to
   lock up in some situations when running macros in IR Standalone mode.
2. Added support for Scrolling Lists.  You must upgrade TheaterTouch
   Designer to version 5.0 or higher to use the Scrolling List support.
3. Increased reliability of double-click tests in macros, and fixed bug
   that caused Press & Hold tests in macros to malfunction when used with
   the Guide key.
4. Assorted performance improvements.

LIST OF CHANGES IN RELEASE 1.3
n/a
(this release was never available as an upgrade, it was issued to support
hardware changes in some T3 units)
 
LIST OF CHANGES IN RELEASE 1.2
1. Fixed issue that could cause the T3 to lock up in some situations when
   a macro contained only a single IR code and no other steps.
2. Fixed issue that prevented macro flags from working in some situations.

LIST OF CHANGES IN RELEASE 1.1
1. Fixed issue that could cause the T3 to lock up in some situations when
   buttons contained both a page link and an IR code or macro.
2. Fixed issue that caused backgrounds with an alpha channel to be
   displayed upside down.
