RTI T3-V+ Firmware Version 1.6.6

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 1.6.6 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer or Integration Designer
to determine the current firmware version. The reported version number
will consist of a number followed by a bootloader version number
[for example: 1.6.6 (Bootloader: 1.5)]. If the first part of the reported
version number is 1.6.6 or higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher, or Integration Designer 6.0 or
higher must already be installed on the PC that you wish to use to
upgrade the T3-V+ firmware.  If your PC runs a 64-bit version of Windows,
Integration Designer 7.0 must be installed to perform the upgrade.
Upgrading to the latest version of Integration Designer is strongly
recommended.  You should verify that you can communicate with the T3-V+
using Integration Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Make sure the battery on the T3-V+ is fully charged.  The T3-V+ may be left
   inoperable if the battery fails during the firmware update.
2. Make sure TheaterTouch Designer 3.0 or higher is installed on the PC
   that you are using to update the T3-V+ firmware, and that TheaterTouch
   Designer can communicate successfully with the T3-V+.  You can use the
   "Get Firmware Version" command on the Communications menu in
   TheaterTouch Designer to verify that the USB communications are
   working properly.
3. Run the T3V+Update_1.6.6.exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

LIST OF CHANGES IN THIS RELEASE (RELEASE 1.6)
1. Fixes intermittent lock-up issues

LIST OF CHANGES IN RELEASE 1.5
1. Fixes potential problem on T3-V+ where the unit can possibly lose Zigbee control
2. Fixes for some MJPG cameras (Sony, Panasonic)

LIST OF CHANGES IN RELEASE 1.4
1. Fix for RM433 cable length issue.
2. Support  for 433MHz RF and Wifi only configuration.
3. Fix for crash when multiple system vars are attached to an item list.
4. Fix for remote wakes up every 20 seconds.
5. Fix for crash when using standalone macros.
6. Fix for lock-up when using standalone macros.
7. Fix for memory leak lock-up when using standalone macros.
8. Fix for 433RF stops working.
9. Fix for dialog box that appears when remote crashes.
10. Fix for double scrolling when two system variables are attached to an item list.
11. Fix for scrollbars showing in browser object regardless of setting.
